


Worksite Safety Inspection – Checklist
	INSTRUCTIONS: Inspections are conducted while work is being performed. When completing inspections, verify compliance with your company’s safety program, and identify unsafe acts or conditions and adherence to applicable Legislation.
This form is designed to support your COR®/SECOR™ audit requirements and can be customized with your organization's branding and site-specific hazards.
For more information on your legal obligations regarding worksite safety please contact us.
INFO@SCSAONLINE.CA or Toll Free 1.800.817.2079



	Company Name:
	Date:
	Time:
	 AM     
 PM

	Project/Site Name:
	Previous Inspection Reviewed:     Yes      No

	Site Address:
	Weather Conditions:

	Area Inspected:
	Site Supervisor:

	Inspection Performed By 
(Supervisor, worker(s) & OHC should be involved)

	
	Print Name
	Position
	Signature

	Lead Inspector: 
	
	
	

	Inspector(s):
	
	
	

	
	
	
	


	General Safety Requirements
	Yes
	No
	N/A
	Fatal FOUR
	Yes
	No
	N/A

	Site safety board is visible with up-to-date information, including: 
	
	
	
	Fall Prevention (Working at Heights)
	
	
	

	Company Safety & Health Policy
	
	
	
	Fall Pro Plan (documented)
	
	
	

	OHC meeting minutes
	
	
	
	Proof of Training 
	
	
	

	OHC list of member representatives
	
	
	
	Equipment – Inspected prior to use
	
	
	

	First Aid Personnel
	
	
	
	Floor openings covered
	
	
	

	Harassment & Violence policy
	
	
	
	Tied off to proper anchor points
	
	
	

	Emergency Response Plan & Contacts
	
	
	
	Ladders properly setup with a 4:1 angle, and 1 metre above the landing
	
	
	

	
	
	
	
	Ladders properly secured and stable
	
	
	

	
	
	
	
	Ladders used correctly (3-points of contact) with proper access & egress
	
	
	

	
	
	
	
	
	
	
	

	The following are up to date and readily available: 
	
	
	
	Struck By Hazards
	
	
	

	Safety & Health Manual 
	
	
	
	High-visibility apparel used around moving equipment and traffic.
	
	
	

	OHS Legislation
	
	
	
	Heavy equipment operators have clear visibility
	
	
	

	Safety Data Sheets
	
	
	
	Spotters used when necessary
	
	
	

	
	
	
	
	Materials stored and stacked safely 
	
	
	

	Other General Safety Requirements
	
	
	
	
	
	
	

	First Aid Kits/Facilities (stocked, accessible)
	
	
	
	Caught-In or Between Hazards
	
	
	

	Eye Wash Stations (available and fully equipped)
	
	
	
	Safety guards are in place on all tools and equipment 
	
	
	

	Fire Extinguishers (inspected, charged, readily available with tag) 
	
	
	
	Lockout/Tagout (LOTO) procedures are followed 
	
	
	

	Emergency Exits (visible/obscured) 
	
	
	
	Workers maintain a safe distance from the swing radius of heavy equipment, i.e.) cranes, PME
	
	
	

	Housekeeping (walkways/ work areas are clear of debris and trip hazards)
	
	
	
	
	
	
	

	Storage areas (tidy, labelled, and appropriate for materials)
	
	
	
	Electrical/ Electrocution Hazards
	
	
	

	Workers have received site-specific safety orientation.
	
	
	
	Minimum clearance distance identified and maintained (from power lines)
	
	
	

	PPE inspected, in good condition, and suitable & properly worn
	
	
	
	Extension cords and electrical tools are inspected for damage (frayed wires, missing ground prongs).
	
	
	

	Hazard Assessments completed
	
	
	
	
	
	
	

	Accidents/Incidents/Near Misses reported and corrective measures implemented 
	
	
	
	Ground Fault Circuit Interrupters (GFCIs) - used for all temporary power outlets.
	
	
	

	Others:
	
	
	
	Use of intrinsically safe devices where required
	
	
	

	
	
	
	
	Temporary lighting - guarded
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	High-Risk Activities
	
	
	

	
	
	
	
	Excavation & Trenching
	Yes
	No 
	N/A

	SITE CONDITIONS
	
	
	
	Underground utilities - located and marked 
	
	
	

	Safe entry and exit 
	
	
	
	Trenches over 1.2 metres (4 ft) deep are sloped, shored, or shielded 
	
	
	

	Muster point identified
	
	
	
	Spoil piles and equipment are kept at least 1 metre (3 ft) back from excavation.
	
	
	

	Noise level acceptable
	
	
	
	
	
	
	

	Housekeeping – slip & trip hazards
	
	
	
	Safe means of access/egress are provided within 8 metres (25 ft) of workers in trenches.
	
	
	

	Adequate lighting
	
	
	
	
	
	
	

	Temperature good
	
	
	
	
	
	
	

	Sanitation facilities available and clean
	
	
	
	Confined Space Entry
	
	
	

	Site parking conditions & signage
	
	
	
	Confined spaces are identified
	
	
	

	Guardrails and barriers 
	
	
	
	Unauthorized entry is prevented
	
	
	

	Traffic Control Plan established & implemented
	
	
	
	Valid entry plan/permit - completed and posted at the entrance.
	
	
	

	
	
	
	
	Atmospheric testing is conducted prior to entry and continuously monitored.
	
	
	

	
	
	
	
	A trained attendant (Stand-by or Watchperson) is present. 
	
	
	

	
	
	
	
	Rescue equipment is readily accessible.
	
	
	

	
	
	
	
	
	
	
	





Details of Deficiencies & Corrective Actions
	RISK MATRIX

	PRIORITY RANKING SCALE INSTRUCTIONS
Evaluate each deficiency using the Priority Index to the right. Select the corresponding number and letter that best fits each deficiency. This will give you your priority ranking, i.e.) 1B. Using the Risk Matrix, you can determine which hazards are high, medium, and low risk. High risk hazards should be addressed immediately, or as soon as possible, while medium and lower risk hazards may be corrected after the inspection is completed.
		
	
	Risk Severity 

	
	
	A (Major Incident/ Fatality)
	B (Medical Aid/ Lost Time)
	C (First Aid/ Near Miss)

	Risk
Probability
	1 (Very Likely)
	High Risk
	High Risk
	Medium Risk

	
	2 (Possible/Likely)
	High Risk
	Medium Risk
	Low Risk

	
	3 (Unlikely) 
	Medium Risk
	Low Risk
	Low Risk






	Deficiency Identified
(Item/Task/Location)
	Priority Ranking
	Corrective Action(s)
Required 
	Assigned To
	Target Date
	Date Completed

	
	
	
	
	
	

	
	
	
	
	
	

	
	


	

	

	

	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	Comments: 


	
	Signature
	
	Date

	Site Supervisor Reviewed
	
	
	

	Management Reviewed
	
	
	


Signatures: Signing indicates review of the inspection findings and commitment to addressing corrective actions.
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