Hazard Assessment Form

Hazard Assessment Form

	Company:
	
	
	Date & Time:
	
	· AM 
· PM
	Project:
	

	Location:
	
	
	Task:
	
	Muster Point:
	
	

	Include site address 
Complete the Hazard Assessment at the task location prior to the start of work and update when conditions change.

	







Radiation: (UV rays, welding arcs, x-rays)





	
Gravity: (falling objects, slip/trip/falls, open holes)






Electrical: (damaged cords, overhead power lines, overloaded circuits)





Biological: (animals, insects, contamination)





	
Motion: (swinging objects, moving equipment/objects/ parts) 






Pressure: (stored energy, mechanical tension, explosions)






Chemical: (flammable, corrosive, toxic materials)





	
Mechanical: (Rotating parts, pinch points, sharp edges)






Sound: (above 85 dBA, loud machinery, vibrations)






Temperature: (heat, cold, burns)






	Instructions: Use information above to complete the Hazard Assessment Form below or on the flip side. 





	PRIORITY INDEX
	Permits & Plans:
	Performing Critical Tasks? (list SWP/SJP below)
 Yes     No

	Probability
	Severity
	
	

	1. Very Likely
	A. Major Incident/Fatality
	 Fall Protection Plan 
	 Lockout/Tagout Permit
	List SWP/SJP Reviewed:



	2. Possible/Likely
	B. Medical Aid/Lost Time
	 Critical Lift Plan
	 Hotwork Permit
	

	3. Unlikely
	C. First Aid/Near Miss
	 Confined Space Permit 
	 Scaffold Inspected
	

	Identify and prioritize the hazards below according to Severity and Probability using a combined risk rating, i.e.) 1A, 2C, etc.

	Tasks 
	Hazards 
(Existing & Potential)
	Priority Ranking
	Control Required
(Provide description)
	Person Implementing Control
	Completed

	
	
	
	
	
	Date
	Time
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	Workers Participation in Hazard Assessment:
	Basic PPE has been inspected and is in good condition?                     Yes     No

	Led by:     Print Name/Initial
	Print Name/Initial
	Hazards Reviewed & Reassessed at:

	Print Name/Initial
	Print Name/Initial
	Time:

	Print Name/Initial
	Print Name/Initial
	Time:

	Print Name/Initial
	Print Name/Initial
	Time:

	Print Name/Initial
	Print Name/Initial
	Time:

	Supervisor Review:
	Print Name/Signature
	Date & Time:
	Supervisor Review
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IMPORTANT: Hazard assessments are conducted before work begins. Existing and potential hazard should be identified with controls implemented prior to starting work activities. When conditions or work being performed changes, the hazard assessment must be updated or a new one completed. For more information on your legal obligations regarding worksite safety, please contact the SCSA.
image1.png





image2.jpeg
gineeri
Controls
Administrative
Controls





